{"text_format":"3","workbook":"xls","n_sheets":7,"sheets":["设备报价表","主要零部件及易损件报价","设备配置及技术参数要求表","供应商服务要求表","招标设备主要部件（主要材料）、主要辅助材料清单表","技术规格偏离表","设备年度招标供应商资质要求"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"设备报价表","index":0,"n_rows":6,"n_cols":6,"rows_kept":6,"merged":[[0,0,0,6],[1,0,2,0],[1,2,1,6],[3,1,5,1]],"flags":["formulas_cached_only"]}
["设备投标报价表"]
["设备单品名称","招标方要求","投标单位填写-供应商名称："]
[null,"招标品牌/型号规格/其他要求","响应品牌","响应型号","单价（元）","偏离描述"]
["无线AP","思科、H3C、优科ruckus、Aruba（或企业无线网络市场占有率前四名的品牌）"]
["AP控制器"]
["用户升级许可（100）"]

{"sheet":"主要零部件及易损件报价","index":1,"n_rows":3,"n_cols":6,"rows_kept":3,"merged":[[0,0,0,5],[1,0,2,0],[1,2,1,5]],"flags":["formulas_cached_only"]}
["主要零部件和易损件报价表"]
["名称（投标单位自行填写）","招标方要求：","投标单位填写-供应商名称："]
[null,"招标品牌/规格型号/其他（由招标方填写）","型号响应","品牌响应","单价","偏离描述"]

{"sheet":"设备配置及技术参数要求表","index":2,"n_rows":39,"n_cols":4,"rows_kept":39,"merged":[[0,0,0,3],[1,0,2,0],[1,2,1,3],[3,0,15,0],[16,0,38,0]],"flags":["formulas_cached_only"]}
["设备配置及技术参数要求表"]
["技术项目","招标方要求","投标单位填写-供应商名称："]
[null,"技术项目要求详细描述（由招标方填写）","对招标要求响应情况具体描述：","偏离描述"]
["无线控制器","虚拟化部署，集团集中管控AP"]
[null,"单台控制AP数量≥1000"]
[null,"支持用户端数量≥25,000"]
[null,"SSID数量≥16"]
[null,"为受控AP自动设置频道和终端服务"]
[null,"根据用户数量的AP负载均衡"]
[null,"控制器故障不影响AP正常工作"]
[null,"二、三层无缝漫游"]
[null,"支持802.1d生成树协议"]
[null,"多控制器配置与管理"]
[null,"WEB用户界面，支持多用户分区管理AP"]
[null,"SNMP v1 v2 v3协议满足"]
[null,"多种报表支持无线网络维护"]
["无线接入点","支持频率2.4G/5G"]
[null,"支持IEEE 802.11a/b/g/n/ac"]
[null,"射频链不低于2 x 2"]
[null,"空间串流不少于2"]
[null,"并发连接用户数≥100"]
[null,"最大 PHY 速率"]
[null,"300 Mbps (2.4GHz)"]
[null,"867 Mbps (5GHz)"]
[null,"1 个自动 MDX、自动感应 10/100/1000 Mbps、RJ-45、 PoE 端口"]
[null,"SNMP（v1/v2c）远程配置和管理"]
[null,"物理天线增益"]
[null,"每空间流最高可达 3 dBi"]
[null,"支持40-bit，128-bit 有线等效加密 (WEP)；WiFi保护存取（WPA-PSK, WPA2-PSK）"]
[null,"无线安全性"]
[null,"WPA-PSK，WPA-TKIP，WPA2 AES，802.11i"]
[null,"使用本地身份认证数据库802.1x 进行身份认证"]
[null,"支持 RADIUS、LDAP 和活动目录"]
[null,"支持集团集中部署"]
[null,"SSID每个接入点不少于 16 个"]
[null,"支持多 VLAN 配置"]
[null,"最大功率输出"]
[null,"对于 2.4GHz†，为 23dBm"]
[null,"对于 5GHz†，则为 24dBm"]

{"sheet":"供应商服务要求表","index":3,"n_rows":16,"n_cols":4,"rows_kept":16,"merged":[[0,0,0,3],[1,0,2,0],[1,2,1,3],[12,0,15,0]],"flags":["formulas_cached_only"]}
["供应商服务要求表"]
["服务项目","招标方要求","投标单位填写-供应商名称："]
[null,"项目要求详细描述","供应商对招标要求响应描述：","偏离描述"]
["赠送条款","无"]
["免费质保期","免费保修不低于3年，且免费提供软件及软件版本升级服务"]
["交货期和交货地点","供应商收到订单或合同签订后10日内到货，交货地点由甲方指定"]
["响应时间","7*24小时相应"]
["付款","按合同所规定的全部货物到货并安装调试至正常使用，并经甲方确认无误后，乙方向甲方提供送货单、全额发票、合同复印件及有甲方签字盖章的验收单，甲方在收到正确付款资料后30个工作日内支付乙方合同总额的95%；剩余5%为质保金，保修期满后支付质保金；之前有合作的供应商可在到货验收后支付全额货款；"]
["售后服务","免费质保期内提供7*24小时上门服务；投标方在国内一线城市均需设有服务网点，网点服务人员不低于2人                                               质保期内如货物经过3次维修仍不能达到正常使用标准，则投标方免费更换合同内合格产品；因人为原因造成的损坏，由投标方负责免费维修，但更换的零配件费用由招标方承担或招标方自行购置零配件；售后服务响应时间不超过1个工作日，若不能用传真及电话解决，投标方应在2个工作日内派人到现场解决问题，如果在2个工作日内无法解决问题，需提供备机。投标方需建立设备维护维修记录和档案，并由双方签字确认；在质保期内，如需返修产品货运费由投标方全部承担；在质保期外，对损坏的配件在接到甲方通知的8小时内给予解决报价，价格不得高于市场价格及与甲方商议时的投标价格。并且在15天内进行更换到位；在质保期外，返修产品返回维修货运费由乙方承担，发回使用由甲方承担货运费。"]
["配件要求","提供设备的配件必须在6年内都有配件进行更换，供货周期不得超过5天。"]
["培训要求","投标方需提供免费培训，并应积极配合招标方的人力培训计划，对所提供的设备进行操作、维护等不同层次的培训工作，并提供相关培训资料。培训次数为每年不低于1次/年，培训时间和地点由双方另行协商。"]
["安装及验收","招标方负责安装设备，投标方做技术支持"]
["其他要求","免费提供软件版本的升级，并提供技术支持"]
[null,"报价需含17%增值税"]
[null,"产品送货上门，并安装。安装地点和方式由招标方确认。调试由招标方完成。"]
[null,"4、中标方必须对其提供的所有产品8年内包修。招标方可选择续签年保或按次维修的方式。年保价格双方协商而定，按次维修只收取配件费。"]

{"sheet":"招标设备主要部件（主要材料）、主要辅助材料清单表","index":4,"n_rows":14,"n_cols":9,"rows_kept":14,"merged":[[0,0,0,8],[1,0,1,8],[3,0,3,8],[8,0,8,8],[13,0,13,8]],"flags":["formulas_cached_only"]}
[" 招标设备主要部件（主要材料）、主要辅助材料清单表"]
["投标单位全称："]
["序号","名称","品牌/型号","制造商","国籍","技术参数","详细性能描述","采购设备配置要求","具体偏离  内容、范围"]
["主要部件："]
[]
[]
[]
[]
["主要材料："]
[]
[]
[]
[]
["辅助材料："]

{"sheet":"技术规格偏离表","index":5,"n_rows":8,"n_cols":7,"rows_kept":8,"merged":[[0,0,0,6],[1,0,1,6],[7,0,7,6]],"flags":["formulas_cached_only"]}
["技术规格偏离表"]
["投标单位全称："]
["序号","名称","招标文件条目号","招标规格","投标规格","偏离","说明"]
[]
[]
[]
[]
["说明：如投标文件与招标文件要求一致，可说明无偏离。"]

{"sheet":"设备年度招标供应商资质要求","index":6,"n_rows":11,"n_cols":12,"rows_kept":11,"merged":[[0,0,0,11],[1,0,1,11],[2,0,2,11],[3,0,3,11],[4,0,4,11],[5,0,5,10],[5,11,7,11],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,7,4],[6,5,7,5],[6,6,7,6],[6,7,7,7],[6,8,7,8],[6,9,7,9],[6,10,7,10],[10,0,10,11]],"flags":["formulas_cached_only"]}
["供应商资质要求表"]
["设备年度招标供应商资质要求"]
["招标项目："]
["投标单位全称："]
["联系人、电话、邮箱："]
["供应商基本要求：",{"$nulls":10},"备注"]
[null,"企业注册资金要求（万元）","企业员工人数要求","年销售额要求","市场占有率要求","企业经营面积要求","企业成立时间要求","主要检测设备要求","主要生产产品要求","研发人员要求","认证资质要求"]
[]
["招标方要求",200,5,"1000万","主流产品",100,"无","无","厂家或核心代理商","无","代理商资质"]
["投标方填写"]
["投标单位填写注意事项：                                                                                                  按照以上项目填写，不要删除行和列，不需要填写的空白即可。此表以电子版存入优盘与招标资质资料一并提交。"]