{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["报价表","材质、制作工艺及技术参数要求表","供应商服务要求表","技术规格偏离表","年度招标供应商资质要求"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"报价表","index":0,"n_rows":12,"n_cols":10,"rows_kept":12,"merged":[[0,0,0,9],[1,0,1,5],[1,6,1,9]],"flags":["formulas_cached_only"]}
["2019年全国各门店需求的PVC、PE保鲜膜类投标报价表"]
["招标方要求",{"$nulls":5},"投标单位填写-供应商名称："]
[null,"商品名称","商品规格","包装","单位"," 上年度价格","响应品牌","响应型号","单价（元）","偏离描述"]
[null,"PVC保鲜膜350*0.011mm*500m","350mm*0.011mm*500m",6,"卷"]
[null,"PE保鲜膜350*0.011mm*500m","350MM*0.011mm*500m",6,"卷"]
[null,"FIT机用PVC保鲜膜","400mm*1000m",2,"卷"]
[null,"保鲜膜捆菜机20.5*13","205mm*130mm",1,"台"]
[null,"捆菜膜宽4cm长200m","40mm*200m",42,"卷"]
[null,"锁鲜装35","20cm*14cm*35cm",600,"只"]
[null,"锁鲜装50","20cm*14cm*50cm",600,"只"]
[null,"PE复合彩印封口膜","膜宽39.3cm直径30cm/卷",1,"kg"]
[null,"PE透明锁鲜包装封口膜","膜宽39.3cm直径30cm/卷",1,"kg"]

{"sheet":"材质、制作工艺及技术参数要求表","index":1,"n_rows":13,"n_cols":8,"rows_kept":13,"merged":[[0,0,0,7],[1,0,1,3],[1,6,1,7],[2,0,2,3]],"flags":["formulas_cached_only"]}
["PVC、PE保鲜膜类材质及制作要求表"]
["招标方要求",{"$nulls":5},"投标单位填写-供应商名称："]
["技术项目要求详细描述（由招标方填写）"]
["名称","规格","材质要求","材料、制作、工艺要求","误差","其他","对招标要求响应情况详细描述：","偏离描述"]
["PVC保鲜膜350*0.011mm*500m","350MM*0.011mm*500m（宽*厚*长）","PVC","材料：聚氯乙烯工艺：流延","膜宽+4mm   膜厚+0.003mm","耐热温度：100℃\n耐热温度：-40℃                  产品要求：表面平整，允许有少量的活褶；色泽正常，无异味，无异嗅，无异物；自粘性强，拉伸强度强，防雾透光性强；\n包装要求：包装牢靠无破损，包装应有产品名称、型号、数量、生产日期、保质期、厂名、厂址及其它符号等中文标注.\n\n成品合格率：100%\n\n"]
["PE保鲜膜350*0.011mm*500m","350MM*0.011mm*500m（宽*厚*长）","PE","材料：聚乙烯","膜宽+4mm   膜厚+0.003mm","耐热温度：100℃\n耐冷温度：-40℃\n\n产品要求：表面平整，允许有少量的活褶；色泽正常，无异味，无异嗅，无异物；自粘性强，拉伸强度强，防雾透光性强； \n包装要求：包装牢靠无破损，包装应有产品名称、型号、数量、生产日期、保质期、厂名、厂址及其它符号等中文标注.\n产品检验依据：通过GB 10457-1989《聚乙烯自粘保鲜膜》\n成品合格率：100%\n\n"]
["FIT机用PVC保鲜膜","400mm*1000m","PVC","材料：聚氯乙烯工艺：流延"]
["保鲜膜捆菜机20.5*13","205mm*130mm"]
["捆菜膜宽4cm长200m","40mm*200m","PVC","材料：聚氯乙烯"]
["锁鲜装35","20cm*14cm*35cm","PP","材料：聚丙烯"]
["锁鲜装50","20cm*14cm*50cm","PP","材料：聚丙烯"]
["PE复合彩印封口膜","膜宽39.3cm直径30cm/卷","PE","材料：聚乙烯"]
["PE透明锁鲜包装封口膜","膜宽39.3cm直径30cm/卷","PE","材料：聚乙烯"]

{"sheet":"供应商服务要求表","index":2,"n_rows":15,"n_cols":4,"rows_kept":15,"merged":[[0,0,0,3],[1,0,2,0],[1,2,1,3]],"flags":["formulas_cached_only"]}
["供应商服务要求表"]
["服务项目","招标方要求","投标单位填写-供应商名称："]
[null,"项目要求详细描述","供应商对招标要求响应描述：","偏离描述"]
["赠送条款","无"]
["免费质保期","无"]
["交货期和交货地点","订单生成后10天内送货；人人乐各分公司配送中心和各门店"]
["响应时间","采用订单方式订货，要求订单生成后10天内送货，如未按时间送达，每拖延一天，将按订单金额的5%违约赔付，在账款中进行扣除。"]
["付款","月结45天"]
["售后服务","具备全国大型连锁零售业相关服务经验，不退货，质量问题可换货"]
["服务费标准","运输服务费2％，票折扣点2.32%，质量保证金2万元/全国。"]
["…","未经人人乐允许不得转承第三方供货，如有做假立即中止合作，冻结所有货款；"]
["样品","备好与报价相匹配的样品，在招标方提出送样两个工作日内科完成"]
["合格率","成品合格率100%"]
["质量标准","投标单位必须保证其产品为合法生产品达到国家规定的质量标准，需具体说明是什么标准"]
["报价成本说明","投标单位必须提供报价及成本分析说明，这将作为评标和最终谈判的重要参考内容；另单独附文字说明"]

{"sheet":"技术规格偏离表","index":3,"n_rows":8,"n_cols":7,"rows_kept":8,"merged":[[0,0,0,6],[1,0,1,6],[7,0,7,6]],"flags":["formulas_cached_only"]}
["技术规格偏离表"]
["投标单位全称："]
["序号","产品名称","招标文件要求","招标规格","投标标准","偏离描述","说明（如正偏离或负偏离"]
[]
[]
[]
[]
["说明：如投标文件与招标文件要求一致，可说明无偏离。"]

{"sheet":"年度招标供应商资质要求","index":4,"n_rows":11,"n_cols":12,"rows_kept":11,"merged":[[0,0,0,11],[1,0,1,11],[2,0,2,11],[3,0,3,11],[4,0,4,11],[5,0,5,10],[5,11,7,11],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,7,4],[6,5,7,5],[6,6,7,6],[6,7,7,7],[6,8,7,8],[6,9,7,9],[6,10,7,10],[10,0,10,11]],"flags":["formulas_cached_only"]}
["                           供应商资质要求表"]
["自用品年度招标供应商资质要求"]
["招标项目：2019年全国各门店需求的PVC、PE保鲜膜类"]
["投标单位全称："]
["联系人、电话、邮箱："]
["供应商基本要求（品类根据各类设备选择以下资质项目，并填写具体要求。如需增加资质项目，加在“备注栏”",{"$nulls":10},"备注"]
[null,"企业注册资金要求（万元）","企业员工人数要求","年销售额要求","市场占有率要求","企业经营面积要求","企业成立时间要求","主要检测要求","主要生产产品要求","研发人员要求","认证资质要求"]
[]
["招标方要求","＞50万　","　＞10人","＞300万,近三年盈利　",{"$nulls":3},"提供产品检测报告","保鲜膜类　","＞1　","　具有制造资质以及国家或行业相关标准"]
["投标方填写"]
["投标单位填写注意事项：                                                                                                  按照以上项目填写，不要删除行和列，不需要填写的空白即可。此表以电子版存入优盘与招标资质资料一并提交。"]